| LiquidMenu 1.2.0 Menu creation Arduino library for LCDs, wraps LiquidCrystal.

B_serial_menu.ino

This example uses the serial communication to execute commands.

/*
* LiquidMenu library - serial_menu.ino
*
* This example uses the serial communication to execute commands.
*
* The available commands will be printed on the serial monitor.
* This example uses attached callback functions which are explained
* in the functions_menu.ino example.
*
* The circuit:
* https://github.com/VasilKalchev/LiquidMenu/blob/master/examples/serial_menu/serial_menu.png
* - LCD RS pin to Arduino pin 12
* - LCD E pin to Arduino pin 11
* - LCD D4 pin to Arduino pin 5
* - LCD D5 pin to Arduino pin 4
* - LCD D6 pin to Arduino pin 3
* - LCD D7 pin to Arduino pin 2
* - LCD R/W pin to ground
* - LCD VSS pin to ground
* - LCD VCC pin to 5V
* - 10k ohm potentiometer: ends to 5V and ground, wiper to LCD V0
* - 150 ohm resistor from 5V to LCD Anode
* - LCD Cathode to ground
*
* Created July 24, 2016
* by Vasil Kalchev
*
* https://github.com/VasilKalchev/LiquidMenu
*
*/
#include <LiquidCrystal.h>
#include <LiquidMenu.h>
// Pin mapping for the display
const byte LCD_RS = 12;
const byte LCD_E = 11;
const byte LCD_D4 = 5;
const byte LCD_D5 = 4;
const byte LCD_D6 = 3;
const byte LCD_D7 = 2;
//LCD R/W pin to ground
//10K potentiometer wiper to VO
LiquidCrystal lcd(LCD_RS, LCD_E, LCD_D4, LCD_D5, LCD_D6, LCD_D7);
LiquidLine welcome_line1(1, 0, "LiquidMenu ", LIQUIDMENU_VERSION);
LiquidLine welcome_line2(1, 1, "Serial example");
LiquidScreen welcome_screen(welcome_line1, welcome_line2);
LiquidLine line21(4, 0, "Screen 2");
LiquidLine type_line(4, 1, "type...");
LiquidScreen screen2(line21, type_line);
LiquidLine line31(4, 0, "Screen 3");
LiquidScreen screen3(line31, type_line);
LiquidLine line41(4, 0, "Screen 4");
LiquidScreen screen4(line41, type_line);
LiquidMenu menu(lcd, welcome_screen, screen2, screen3, screen4);
/*
* This function will be attached to one or more LiquidLine
* objects and will be called when the line is focused and
* bool LiquidMenu::call_function(byte number) is called with
* number - the number specified when attaching the function.
* More on this in the function_menu.ino example.
*/
void callback_function() {
Serial.println("You called the callback function.");
}
void setup() {
Serial.begin(250000);
lcd.begin(16, 2);
// Here we attach the function defined earlier to four LiquidLine objects.
line21.attach_function(1, callback_function);
line31.attach_function(1, callback_function);
line41.attach_function(1, callback_function);
type_line.attach_function(1, callback_function);
menu.update();
Serial.print("LiquidMenu "); Serial.print(LIQUIDMENU_VERSION); Serial.println(" - Serial example:");
Serial.println("To navigate the menu type 'menu.next_screen()' or 'menu.previous_screen()'.");
Serial.println("To switch focus type 'menu.switch_focus()'.");
Serial.println("To call the callback function type 'menu.call_function(1)'.");
Serial.println("To adjust the focus position type 'menu.set_focusPosition(Position::LEFT)'");
Serial.println(" or 'menu.set_focusPosition(Position::RIGHT)'.");
Serial.println("To update the display type 'menu.update()'."); Serial.println();
}
void loop() {
// This handles the serial input.
while (Serial.available() > 0) {
String command = Serial.readStringUntil('\0');
if (command == "menu.next_screen()") {
Serial.println(command);
menu.next_screen();
} else if (command == "menu.previous_screen()") {
Serial.println(command);
menu.previous_screen();
} else if (command == "menu.switch_focus()") {
Serial.println(command);
menu.switch_focus(); // switches focus to the next line
// focus is used with functions (see 'functions_menu' example)
} else if (command == "menu.call_function(1)") {
Serial.println(command);
// The attached function is called.
menu.call_function(1);
} else if (command == "menu.set_focusPosition(Position::LEFT)") {
Serial.println(command);
// this function sets the focus position
menu.set_focusPosition(Position::LEFT);
} else if (command == "menu.set_focusPosition(Position::RIGHT)") {
Serial.println(command);
menu.set_focusPosition(Position::RIGHT);
} else if (command == "menu.update()") {
Serial.println(command);
menu.update();
} else {
Serial.print(command); Serial.println(" - unknown command");
}
menu.update();
}
}