| LiquidMenu 1.3.0 Menu creation Arduino library for LCDs, wraps LiquidCrystal.

Macros | Variables
LiquidMenu_config.h File Reference

Go to the source code of this file.

## Macros
#define | I2C false
| Switches the communication method to I2C. More...
#define | LIQUIDMENU_DEBUG false

## Variables
const uint8_t | MAX_VARIABLES = 5
| Configures the number of available variables per line. More...
const uint8_t | MAX_FUNCTIONS = 8
| Configures the number of available functions per line. More...
const uint8_t | MAX_LINES = 12
| Configures the number of available lines per screen. More...
const uint8_t | MAX_SCREENS = 14
| Configures the number of available screens per menu. More...
const uint8_t | MAX_MENUS = 8
| Configures the number of available menus per menus system. More...

## Detailed Description

Configuration file for LiquidMenu library.

Contains global constants the configure the size of some of the arrays used in the library, also configures the debugging messages.

## Macro Definition Documentation

## § I2C

#define I2C false

Switches the communication method to I2C.

Note
  Default: false

## § LIQUIDMENU_DEBUG

#define LIQUIDMENU_DEBUG false

Note
  Default: false

## Variable Documentation

## § MAX_FUNCTIONS

const uint8_t MAX_FUNCTIONS = 8

Configures the number of available functions per line.

Note
  Default: 8

## § MAX_LINES

const uint8_t MAX_LINES = 12

Configures the number of available lines per screen.

Note
  Default: 12

## § MAX_MENUS

const uint8_t MAX_MENUS = 8

Configures the number of available menus per menus system.

Note
  Default: 8

## § MAX_SCREENS

const uint8_t MAX_SCREENS = 14

Configures the number of available screens per menu.

Note
  Default: 14

## § MAX_VARIABLES

const uint8_t MAX_VARIABLES = 5

Configures the number of available variables per line.

Note
  Default: 5